[image: ]Commonly used screw conceyor specifications comparison table
	
	Φ168
	Φ219
	Φ273
	Φ323
	Φ407

	
	24t/h
	40 t/h
	80 t/h
	110 t/h
	170 t/h

	2
	1500-5-28-4
	1500-5-28-4
	2000-7-38-5.5
	2000-7-38-7.5
	3000-10-42-15

	3
	1500-5-28-4
	1500-5-28-4
	2000-7-38-5.5
	2000-7-38-7.5
	3000-10-42-15

	4
	1500-5-28-4
	1500-5-38-5.5
	2000-7-38-7.5
	2000-7-42-11
	3000-10-42-15

	5
	1500-5-28-4
	1500-5-38-5.5
	2000-7-38-7.5
	2000-7-42-11
	3000-10-42-15

	6
	1500-5-38-5.5
	1500-5-38-7.5
	2000-7-42-11
	3000-10-42-15
	3000-10-48-18.5

	7
	1500-5-38-5.5
	1500-5-38-7.5
	2000-7-42-11
	3000-10-48-18.5
	3000-10-48-18.5

	8
	1500-5-38-7.5
	1500-5-42-11
	2000-7-42-15
	3000-10-48-18.5
	3000-10-48-22

	9
	1500-5-38-7.5
	1500-5-42-11
	2000-7-42-15
	3000-10-48-22
	3000-10-48-22

	10
	1500-5-38-7.5
	1500-5-42-11
	2000-7-42-15
	3000-10-48-22
	3000-10-48-30

	11
	1500-5-38-7.5
	1500-5-42-11
	3000-7-42-15
	3000-10-48-22
	3000-10-48-30

	12
	1500-5-38-7.5
	1500-5-42-11
	3000-7-48-18.5
	3000-10-48-22
	3000-10-48-30

	13
	1500-5-38-7.5
	1500-5-42-15
	3000-7-48-18.5
	3000-10-48-30
	3000-10-48-30

	14
	1500-5-38-7.5
	1500-5-42-15
	3000-7-48-18.5
	3000-10-48-30
	

	15
	
	1500-5-42-15
	3000-7-48-18.5
	3000-10-48-30
	


Note: 1. The meaning of the numbers in the table is: reducer model - transmission ratio - input shaft diameter - motor power
[bookmark: _GoBack]2. When the effective length of the screw conveyor is greater than or equal to L+05m, the upper limit power is used. When the effective length is less than L+0.5m, the upper limit power is used.
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